# Virtual LANs

The term VLAN (Virtual Local Area Network) refers to a collection of devices that communicate as if they were on the same physical LAN. Any set of ports (including all ports on the switch) can be considered a VLAN. LAN segments are not restricted by the hardware that physically connects them.

| VLANs offer the ability to group computers together into logical workgroups. This can simplify network administration when connecting clients to servers that are geographically dispersed across the building, campus, or enterprise network. Typically, VLANs consist of co-workers within the same department but in different locations, groups of users running the same network protocol, or a cross-functional team working on a joint project.

By using VLANs on your network, you can:

- Improve network performance

- Limit broadcast storms

- Improve LAN configuration updates (adds, moves, and changes)

- Minimize security problems

- Ease your management task

## Other Considerations

- To set up IEEE VLAN membership (multiple VLANs), the adapter must be attached to a switch with IEEE 802.1Q VLAN capability.

- A maximum of 64 VLANs per network port or team are supported by Intel software.

- VLANs can co-exist with teaming (if the adapter supports both). If you do this, the team must be defined first, then you can set up your VLAN.

- The Intel PRO/100 VE and VM Desktop Adapters and Network Connections can be used in a switch based VLAN but do not support IEEE Tagging.

- You can set up only one untagged VLAN per adapter or team. You must have at least one tagged VLAN before you can set up an untagged VLAN.

| CAUTION: When using IEEE 802 VLANs, settings must match between the switch and those adapters using the VLANs.

# Configuring VLANs in Microsoft* Windows*

In Microsoft* Windows*, you must use Intel® PROSet to set up and configure VLANs. For more information, select Intel PROSet in the Table of Contents (left pane) of this window.

| Note: If you change a setting under the Advanced tab for one VLAN, it changes the settings for all VLANS using that port.

The following versions of Microsoft Windows support Intel Network Adapters when configured for VLANs:

- Windows 2000 (with Service Pack 4 or later)

- Windows XP

- Windows Vista*

- Windows Server* 2003

- Windows Server 2008

In most environments, a maximum of 64 VLANs per network port or team are supported by Intel PROSet.

`Last modified on 12/11/07 4:13p Revision 15`